Wi-SUN Network Test Report

# Test Information

|  |  |
| --- | --- |
| Test Type: | AVAILABILITY |
| Started: | 2025-10-16 18:47:50 |
| Format: | Word Document |

# Test Results

# Test Results

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Sr No.** | **IP Address** | **Device Label** | **Hop Count** | **Availability Status** | **Connection Status** |
| 1 | FD12:3456::B635:22FF:FE98:2537 | WN-L031-30 | 1 | 97.09% | AVAILABLE |
| 2 | FD12:3456::B635:22FF:FE98:2523 | WN-L032-30 | 2 | 93.94% | AVAILABLE |
| 3 | FD12:3456::B635:22FF:FE98:252B | WN-L033-30 | - | No response or CoAP error | UNAVAILABLE |
| 4 | FD12:3456::62A4:23FF:FE37:A3B3 | WN-L034-30 | 2 | 93.05% | AVAILABLE |
| 5 | FD12:3456::B635:22FF:FE98:285B | WN-L035-30 | 3 | 93.66% | AVAILABLE |
| 6 | FD12:3456::62A4:23FF:FE37:A3A1 | WN-L036-30 | - | No response or CoAP error | UNAVAILABLE |
| 7 | FD12:3456::B635:22FF:FE98:2539 | WN-L037-30 | 4 | 92.33% | AVAILABLE |
| 8 | FD12:3456::B635:22FF:FE98:285C | WN-OF04-34 | 2 | 96.29% | AVAILABLE |
| 9 | FD12:3456::92FD:9FFF:FEEE:9DF7 | WN-L050-30 | 2 | 93.27% | AVAILABLE |
| 10 | FD12:3456::B635:22FF:FE98:285D | WN-L051-30 | 2 | 93.45% | AVAILABLE |
| 11 | FD12:3456::B635:22FF:FE98:253F | WN-L038-30 | 3 | 89.92% | UNAVAILABLE |
| 12 | FD12:3456::62A4:23FF:FE37:A3A8 | WN-L039-30 | 7 | 91.67% | AVAILABLE |
| 13 | FD12:3456::B635:22FF:FE98:2541 | WN-L040-30 | - | No response or CoAP error | UNAVAILABLE |
| 14 | FD12:3456::B635:22FF:FE98:2529 | WN-L041-30 | 6 | 91.53% | AVAILABLE |
| 15 | FD12:3456::62A4:23FF:FE37:A3AC | WN-L042-30 | 7 | 81.06% | UNAVAILABLE |
| 16 | FD12:3456::62A4:23FF:FE37:A39F | WN-L043-30 | 6 | No response or CoAP error | UNAVAILABLE |
| 17 | FD12:3456::B635:22FF:FE98:2534 | WN-L044-30 | 6 | No response or CoAP error | UNAVAILABLE |
| 18 | FD12:3456::B635:22FF:FE98:2524 | WN-L045-30 | - | No response or CoAP error | UNAVAILABLE |
| 19 | FD12:3456::92FD:9FFF:FEEE:9D40 | WN-L047-30 | 5 | 92.03% | AVAILABLE |
| 20 | FD12:3456::B635:22FF:FE98:29A6 | WN-L048-30 | 2 | 100.0% | AVAILABLE |
| 21 | FD12:3456::62A4:23FF:FE37:A3AD | WN-L052-30 | 5 | 68.63% | UNAVAILABLE |
| 22 | FD12:3456::B635:22FF:FE98:252C | WN-L053-30 | 4 | 71.41% | UNAVAILABLE |
| 23 | FD12:3456::B635:22FF:FE98:251E | WN-L054-30 | 3 | 66.41% | UNAVAILABLE |
| 24 | FD12:3456::B635:22FF:FE98:253E | WN-VA24-30 | 3 | 95.97% | AVAILABLE |
| 25 | FD12:3456::B635:22FF:FE98:285E | WN-VA64-30 | 1 | 97.73% | AVAILABLE |
| 26 | FD12:3456::62A4:23FF:FE37:A3A9 | WN-VC44-30 | 1 | 97.81% | AVAILABLE |
| 27 | FD12:3456::62A4:23FF:FE37:A3AB | WN-NI04-34 | - | No response or CoAP error | UNAVAILABLE |
| 28 | FD12:3456::B635:22FF:FE98:29A5 | WN-L059-34 | 3 | 67.49% | UNAVAILABLE |